INOPERATIVE SPEEDOMETER TRANSMISSION INFORMATION. Buick Electra Limited 1984

For 1990-2009 cars

# INOPERATIVE SPEEDOMETER TRANSMISSION INFORMATION

#### Models Affected: 1984 Regal, Lesabre and Electra with 200-4R Transmission

You may encounter a condition where the plastic speedometer driven gear sleeve contacted the teeth of the drive gear. Wear from this condition, may result in gear tooth clearance between the gears, resulting in an inoperative speedometer.

The correction of this condition is to replace the plastic speedometer sleeve with a steel sleeve, part no. 25519848. Inspect the drive and driven gears for any damage and replace if necessary.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.