RESTRICTED EXHAUST PLUGGED CATALYTIC CONVERTER. Buick Electra Estate Wagon 1983

For 1990-2009 cars

# RESTRICTED EXHAUST PLUGGED CATALYTIC CONVERTER

#### MODELS AFFECTED: 1983 EQUIPPED WITH 4.1L (VIN CODE 4) V-6 ENGINES

Some 1983 Buicks produced prior to March 1983 and equipped with 4.1L V-6 engines may develop a restricted exhaust due to the catalytic converter becoming plugged. This can result in poor engine performance or a no-start condition.

Effective with this bulletin, subject vehicles, which are determined to have a restricted converter, are to be repaired with the converter kit package which includes a converter shell with beads in the upper bed and a plug for sealing the lower bed after installing beads per the instructions in this bulletin.

PARTS INFORMATION

Parts are to be obtained from GMWDD using the following part numbers:

DESCRIPTION PART NUMBER

Kit, Catalytic Converter with Upper 25056983 Beads (Includes converter number 25056905, fill hole plug 8998202 and instruction sheet.)

*Package, Lower Bed Bead 25056903 (As needed to Fill Converter)

Clamp, Converter Front Exhaust 1259609 (If needed)

Bolt, Intermediate Exhaust Pipe to 11502877 Converter (Two per vehicle, if needed)

Bolt, Exhaust Hanger to Converter 11504596 (Two per vehicle, if needed)

*A lower Bed Bead package, when used along with the beads removed from the old converter, will complete approximately ten (10) vehicles.

Additional fill hole plugs, if required, may be ordered using part number 8998202.

SPECIAL TOOLS

A. Converter Bead Replacement Tool Kit

Each Buick dealer was shipped during March 1983, one (1) complete catalytic converter bead replacement tool kit J-34155, no charge. Each kit consists of:

J-34155-1 Sifting Pan (1) J-34155-2 Storage Pans (2) J-34155-3 Funnel (1)

In the event additional kits are required by the dealer, they may be purchased from:

Kent-Moore Tool Division Kent-Moore Corporation 29784 Little Mack Roseville, M.I. 48066

CATALYTIC CONVERTER REPLACEMENT PROCEDURE

#### CAUTION:

The catalytic converter beads contain platinum, palladium, and/or rhodium. Additionally, the beads may be finely coated with lead compounds. Therefore, precautions should be taken to minimize dust generation during the replacement procedure. These precautions include:

Catalyst dust should be controlled by wetting with water prior to bead removal, as described in Step 4.

The use of a suitable dust mask, rubber gloves, and safety glasses is recommended when handling catalyst beads.

Applicable OSHA standards should be reviewed.

Allow converter to cool before handling.

1. Loosen clamp and disconnect AIR pipe from converter.

2. Disconnect intemediate exhaust pipe and hanger from rear of converter.

3. Remove clamp and disconnect converter from front exhaust pipe.

4. Stand the old converter upright on the inlet end and pour 16 ounces of water into the outlet end to control catalyst dust.

5. Using a hammer and chisel, remove the fill hole plug from the lower bed (the smooth side of the converter is the lower bed side). See Figure 1.

6. Hold the converter over a clean pan (J-34155-2) and empty the catalyst beads by shaking. It may be necessary to tap the converter belt flange with a hammer to loosen the beads.

7. Pour the beads into a sifting pan (J-34155-1) and sift to remove undersized beads.

8. Prop the new converter up at a 45-degree angle with the lower bed fill hole at the top.

9. Using funnel J-34155-3, pour the sifted beads into the lower bed of the new converter (see Figure 1). Tap belt flange with rubber mallet to allow beads to settle. Continue filling and tapping until converter is full. If additional beads are required to completely fill the lower bed, it will be necessary to obtain a lower bed bead kit from the parts department. Excess beads from the kit should be saved in a clean container for future use.

10. Lay the converter down on a flat surface with the lower bed fill hole on top.

11. Insert the fill plug into the lower bed fill hole. The fill plug outer rim must rest against the converter body.

12. Insert tool J-34188 into fill plug and tighten to a torque 47 N.m (35 lb. ft.) (see Figure 2).

13. Install new converter in vehicle reversing removal procedure (Steps 1, 2, and 3) and using new bolts and clamp as required. Torque front clamp nuts to 35 N.m (26 lb. ft.), intermediate pipe to converter bolts to 20 N.m (15 lb. ft.) and hanger to converter bolts to 52 N.m (38 lb. ft.).

WARRANTY INFORMATION

Labor Trouble Operation Number Hours Code

T5094 .9 hr. 92

When submitting a warranty claim, the parts amount requested must reflect an amount equal to only the portion of the lower bead package, part number 25056903, used for completing the repair when a complete bead package is not required. When only a portion of the bead package is used, a parts count of one (1) must be included in the total parts count entry.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.