INTERMITTENT HIGH IDLE GROUNDING OF ILC SOLENOID. Buick Electra Estate Wagon 1985

For 1990-2009 cars

# INTERMITTENT HIGH IDLE GROUNDING OF ILC SOLENOID

#### Models Affected: 1985 Lesabres and Rivieras Equipped with a 5.0L Engine (Vin Code Y)

An intermittent idle speed condition most noticeable after extended periods of driving, may occur on some 1985 LeSabre and Riviera models equipped with a 5.0L V-8 engine. This condition may be due to intermittent internal grounding of the idle load compensator solenoid resulting in a loss of vacuum to the idle load conpensator motor. this condition can be repaired by replacing the idle load compensator solenoid.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.