1987 NEW VEHICLE ANNOUNCEMENT BOOKLETS/MANUAL INFORMATION. Buick Electra Estate Wagon 1987

For 1990-2009 cars

# 1987 NEW VEHICLE ANNOUNCEMENT BOOKLETS/MANUAL INFORMATION

#### MODELS AFFECTED: ALL 1987 BUICKS

1. 1987 Warranty and Owner Assistance Information Booklets 2. 1987 Buick Service Manuals 3. 1987 Buick Owner's Manuals 4. 1987 Vehicle Certification and Tire Pressure Label 5. 1987 Service Parts Identification Label 6. 1987 New Vehicle Inspection Procedure Sheets 7. 1987 Buick Passenger Car Maintenance Schedule Booklet 8. 1987 Buick Labor Time Guide 9. 1987 Buick Bulletin Binders 10. 1987 Paint Codes 11. MIC Life Belt Certificate

1. WARRANTY AND OWNER ASSISTANCE ON 1987 BUICK NEW CARS -------------------------------------------------------- The following booklets containing warranty information relative to the new car, emission systems, tire and corrosion are used in 1987:

Part #25531162 - Riviera and FWD Electra/Park Avenue Part #25531161 - All except Riviera and FWD Electra/Park Avenue

Early built cars used Part #25529487 (Riviera and FWD Electra/Park Avenue) and Part #25529486 (All except Riviera and FWD Electra/Park Avenue which should be replaced with booklet of current part number.

Owner assistance satisfaction procedures, the GM mediation/arbitration program, special policy adjustment programs, and the GM Continuous Protection Plan are all outlined in this booklet. A separate tire warranty folder is included to outline warranty as provided by individual tire manufacturers.

The owner's name, address, Vehicle Identification Number, date of delivery and mileage at the time of delivery, are all to be typed on the front cover of the Warranty and Owner Assistance Information booklet in the space provided. There is a space provided on the back of the folder for the dealer name, address and dealer code.

It is very important that the Owner and Vehicle Information on the booklet be correct. This information will be the only means of owner identification for repairs covered under warranty. In order for dealer warranty claims to be properly processed, the Vehicle Identification Number must be correct. Owners should be instructed to carry their Warranty and Owner Assistance Information Booklets in their vehicles at all times.

2. 1987 SERVICE MANUALS ----------------------- The 1987 Chassis Service Manual will be shipped to all Buick dealers in early September, 1986. Again for 1987, it is a loose-leaf publication in two volumes ccvering all models.

Post type binders will be included with each manual.

1987 Fisher Body Manual will be shipped in October, 1986.

Additional manuals and/or binders can be ordered on the "Service Publications for Buick Dealer" order form which is included with the Chassis Service Manual shipment or available from your Zone Office.

3. 1987 OWNER'S MANUALS ---------------------- For 1987 there are a total of eight (8) owner's manuals.

Part # 25529488 - Century Part # 25529489 - LeSabre Estate Wagon/Electra Estate Wagon Part # 25526739 - Electra/Park Avenue Part # 25529491 - Riviera Part # 25527272 - Regal Part # 25526905 - LeSabre Part # 25529490 - Skyhawk Part # 25529493 - Somerset/Skylark

4. 1987 VEHICLE CERTIFICATION AND TIRE PRESSURE LABEL ---------------------------------------------------- In accordance with Federal Motor Vehicle Regulations, A Vehicle Certification and Tire Pressure Label is beirig affixed to all 1987 model Buicks.

The label will have a certification statement, Vehicle Identification Number, month and year that the vehicle was built. The label will be attached horizontally to the left front door inner panel lock facing on all models.

The lower portion of the label will have the tire size and tire pressure information.

Due to the ceritification label's location, it may be subject to damage during car shipment and new vehicle pre-delivery service or may be required due to door repair or replacement.

1987 BUICK EXTERIOR COLORS (EXCEPT OKLAHOMA CITY ASSEMBLY)

SHERWIN- INMONT/ WILLIAMS PAINT SERIES PPG RINSHED (ACME- MARTIN CODE COLOR WA# USAGE DITZLER DUPONT MASON ROGERS) SENOUR ----- ----- --- ------ ------- ------ ------- -------- ------

11 WHITE 3967 A,G,J, 2058 5338 2080 L1OA-2864 30-3929 B-WAGON (5644) 12 SILVER * 8535 A,G,J, 3746 B8501 15001 34380 34-5371 B-WAGON 13S SILVER B/C * 9021 C,E,H, 3822 D8590 15365 35369 30-5491 14 BLACK B/C * 8767 E,H 3961 B8701 17002 35877 35877 15 MED. GRAY * 8573 A,G,J, 3749 B8502 15004 34381 30-3572 B-WAGON 19 BLACK 848 A,G,J, 9000/ 99S PKG L1OB-1738 3069 B-WAGON 9300 (3000/4590)

22 LT. BLUE B/C * 8966 C,E,H,N 3964 B8703 17003 35879 35879 24 BRIGHT BLUE * 8928 J 3883 B8601 16002 35252 30-5471 25 LT. BLUE * 8574 A,G, 3754 B8503 15009 34382 30-5373 B-WAGON 26 LT. SAPPHIRE 8964 J 3966 B8704 17005 35865 35865 BLUE * 27 MED. SAPPHIRE 8742 N 3967 B8705 17004 35882 35882 BLUE B/C * 28 DK. BLUE B/C * 8743 C,E,H 3885 B8618 16003 35313 30-5520 29 DK. SAPPHIRE 8970 J 3968 B8706 17007 35866 35866 BLUE B/C * 31 DK. BLUE * 8592 A,G, 3760 B8504 15014 34875 30-5441 B-WAGON 33 LT. DRIFTWOOD 9022 C,E,H 3970 B8707 17009 35905 35905 B/C * 40 WHITE B/C 8554 C,E,H,N 3680 B8469 13570 33755 30-5295 41 BLACK B/C 8555 C,E,H 9700 99S 13572 33756 30-5296 42 LT. TEAL B/C * 8968 H 3973 B8708 17010 35884 35884 43 LT. TEAL * 8572 A,G, 3762 B8505 15016 34386 30-5377 B-WAGON 48 DK. TEAL B/C * 8747 C,E,H 3888 B8608 16006 35315 30-5482

52 COPPER BEIGE 8973 N 3976 B8710 17014 35887 35887 B/C 54 CREAM BEIGE 8525 A,G,J, 3769 B8521 15023 34861 30-5437 B-WAGON 58 LT. CHESTNUT * 8575 A,G,J, 3772 B8507 15046 34396 30-5387 B-WAGON 62 DK. BROWN * 8593 A,G,J, 3776 B8508 15030 34398 30-5389 B-WAGON 63 LT. DRIFTWOOD 8744 C,E,H 3894 B8603 16011 35310 30-5481 B/C 64 MED. COPPER 8978 N 3982 B8711 17016 35891 35891 B/C * 67 LT. COPPER 8977 N 3984 B8712 17017 35890 35890 B/C *

1987 BUICK EXTERIOR COLORS (EXCEPT OKLAHONA CITY ASSEMBLY)

SHERWIN- INMONT/ WILLIAMS PAINT SERIES PPG RINSHED (ACME- MARTIN CODE COLOR WA# USAGE DITZLER DUPONT MASON ROGERS) SENOUR ----------- --- ------ ------- ------ ------- ------- -------

70 CARMINE 8530 J 3781 B8512 15035 34401 30-5392 71 MED. RED * 8772 A,G, 3899 B8602 16016 35319 30-5484 B-WAGON 72 MED. GARNET 8979 E,H,N 3986 B8713 17021 35894 35894 RED B/C * 76 OK. GARNET 8984 C,E,H 3989 B8716 17023 35895 35895 RED B/C * 78 MED. ROSEWOOD* 8986 J 3991 B8717 17024 35873 35873 79 DK, RED * 8529 A,G, 3786 B8509 15040 34405 30-5396 B-WAGON 80 LT. ROSEWOOD 8992 E,N 3993 B8718 17027 35898 35898 B/C * 82 MED. ROSEWOOD 8990 E,N 3994 B8719 17026 35896 35896 B/C * 83 MED. 8993 C,E 3995 B8720 17028 35900 35900 SAPPHIRE F/M B/C * 84 GUNMETAL B/C * 7782 C,E 3667 B8403 14066 33936 30-5313 86 DK. ROSEWOOD * 8987 J 3996 B8721 17025 35874 35874

92 MED. EMERALD 8931 C 3904 B8607 16022 35255 30-5474 FIREMIST B/C * 96 DK. DRIFTWOOD 8765 C,E 3906 B8605 16024 35324 30-5486 FIREMIST B/C *

B/C - BASECOAT/CLEARCOAT * METALLIC

1987 BUICK EXTERIOR COLORS OKLAHOMA CITY ASSEMBLY - PLANT CODE 6

SHERWIN- INMONT/ WILLIAMS PAINT PPG RINSHED (ACME MARTIN CODE COLOR WA# DITZLER DUPONT MASON -ROGERS) SENOUR ----- ----- --- ------- ------ ------- -------- ------

11 WHITE B/C 9330 3919 D8601 16456 36633 36633 12 SILVER B/C * 9331 3920 D8602 16445 36634 36634 15 GRAY B/C * 9332 3921 D8603 16446 36635 36635 19 BLACK B/C 9333 9000/9300 99S 13572 36636 36636 25 LT. BLUE B/C* 9334 3922 D8604 16447 37382 36637 31 DK. BLUE B/C* 9335 3923 D8605 16448 34875 36638 43 LT. SAGE B/C* 9336 3924 D8606 16449 36639 36639 54 CREAME BEIGE 9337 3925 D8607 16450 36640 36640 B/C * 58 LT. BROWN 9338 3926 D8608 16451 36641 36641 B/C* 62 BROWN B/C * 9339 3927 D8609 16452 36642 36642 71 ROSEWOOD B/C* 9340 3928 D8611 16453 36643 36643 79 DK. RED B/C * 9341 3929 D9610 16454 36644 36644

B/C - BASECOAT/CLEARCOAT * - METALLIC

To acquire a replacement certification label, proceed as follows:

A. Obtain an impression of the Vehicle Identification Number on the engine block by rubbing a pencil lightly over a piece of paper held in place against the block. B. Obtain build date, if at all possible, from damaged certification label. C. Check Vehicle Identification Number on engine block and identification number on instrument panel to see that they match. D. Obtain the vehicle order number from invoice. E. Send the readable impression and build date from Steps A and B above and the vehicle order number taken from the invoice, along with a letter of explanantion to:

Buick Motor Division Attn: Manager - Technical Service Flint, MI 48550

5. SERVICE PARTS IDENTIFICATION LABEL ------------------------------------ Some assembly centers no longer use a Body Number Plate that contains paint and trim information. This information, along with options and build content is now recorded on the Service Parts Identification (SPID) label. Care should be taken to transfer the SPID label or its information, if panel to which label is affixed requires replacement. Replacement SPID labels are not available.

6. 1987 NEW VEHICLE INSPECTION PROCEDURE FORM --------------------------------------------- The New Vehicle Inspection and Delivery Procedure which was introduced in 1983, includes a new NVI for 1987. Use New Vehicle Inspection Procedure Sheet 101072, revised 7/86. This form is shipped with each Buick delivered to you. Additional forms may be obtained through your Zone Office.

7. 1987 MAINTENANCE SCHEDULE ---------------------------- For 1987 there is one (1) vehicle maintenance booklet for all cars, part number 14102712.

8. 1987 LABOR TIME GUIDE - MICROPUBLICATIONS UPDATE AND REQUEST FOR REVIEW FORMS ------------------------------------------------------------------- Approximately September 19, 1986, one (1) set of micropublications will be mailed to all dealers, each set will consist of the following material:

o Labor Time Guide - 1987 (2) o Dealer Information Bulletin Update - October 1983-August 1984 (3) o Dealer Service Bulletin Update - All 1986 (1) o Dealer Campaign Bulletin Update - September 1985-August 1986 (2) o Essential/Available Tool Catalog Update - 1986 (1) o Chassis Service Manual - 1985 (1)

Additional quantities, if previously ordered, will be supplied, based upon records on file at time of mailing. All requests for additional microfiche sets are to be processed directly thru GM Photographic. Additional order forms are available from your Zone Office.

Labor Time Guide - All claims processed on the date of receipt or after will be processed on the basis of operations and labor time allowances provided.

#### Printed Labor Time Guide

The 1987 Labor Time Guide is available in printed format. This loose leaf publication can he ordered on the "Service Publications for Buick Dealers" order form. Binders are also available. Printed Labor Time Guides will automatically be sent to dealers who have previously ordered on a continuing basis.

9. 1987 BUICK BULLETIN BINDERS ------------------------------ Binders and index tabs should be ordered using the "Service Publication for Buick Dealers" order form.

10. 1987 PAINT CODES -------------------- Color chip sheets for the 1987 Buick Paints will again be available from DuPont, Ditzler, Inmont (Rinshed-Mason), Sherwin Williams, Acme/Rogers and Martin-Senour.

The followirg charts indicate 1987 exterior paint supplier stock number, the WA numbers and vehicles the paint is used on. The paint numbers listed in this bulletin along with clearcoat materials, are or soon will be available from local paint suppliers. Please note that the Service Parts Identification Label includes paint information.

When contacting your local paint supplier for repair materials, make sure that you specify the type of material needed. If your paint supplier is unable to provide you with the material needed, ask him to contact his manufacturer sales representative for assistance.

11. MIC LIFE BELT CERTIFICATE ----------------------------- The MIC Life Belt Certificate, Part #14085225, has been discontinued for 1987.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.