REAR STRUT REMOVAL REVISED PROCEDURE. Buick Electra/Park Avenue 1985

For 1990-2009 cars

# REAR STRUT REMOVAL REVISED PROCEDURE

#### VEHICLES AFFECTED: 1985 'C' Series vehicles

The procedure to remove a rear struct from a 1985 'C' series vehicles has been revised. When removing a rear strut, support the control arm with a jack stand prior to removing any strut fasteners.

Please update page 3D-4 of your 1985 chassis service manual with this information.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.