INOPERATIVE D.I.C. CHECK FUSE INSTALLATION. Buick Electra/Park Avenue 1988

For 1990-2009 cars

# INOPERATIVE D.I.C. CHECK FUSE INSTALLATION

DCS NO. 87-24 GROUP NO. 9 TO: ALL BUICK DEALERS ATTN: SERVICE MANAGERS BE SURE TO REVIEW THIS INFORMATION WITH YOUR MAKE READY PERSONNEL SOME EARLY BUILT 1988 PARK AVENUE MODELS WITH THE ELECTRONIC DIGITAL INSTRUMENT CLUSTER (OPTION U52) WERE BUILT WITH THE WRONG FUSE ILLUSTRATION INSTRUCTIONS ON THE REAR VIEW MIRROR FUSE TAG. THE FUSE MUST BE INSTALLED IN NUMBER THREE (3) FUSE LOCATION FOR THE CLUSTER TO FUNCTION PROPERLY. VEHICLES AFFECTED ARE IN SERIAL NUMBER RANGE J1600092 THROUGH AND INCLUDING J1601658. PLEASE MAKE SURE FUSE IS INSTALLED IN LOCATION NUMBER 3 ON ANY VEHICLE WITH U52 OPTION WITHIN ABOVE SERIAL NUMBER RANGE. B. E. ORVIS MANAGER - TECHNICAL SERVICE LWH/GW 8/19/87

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.