ECC POWER MODULE INOPERATIVE COMPRESSOR DIODE LEADS SHORTED. Buick Electra/Park Avenue 1981

For 1990-2009 cars

# ECC POWER MODULE INOPERATIVE COMPRESSOR DIODE LEADS SHORTED

ECC POWER MODULE INOPERATIVE - 1981 C-CAR WITH V-6 THE ECC POWER MODULE MAY BECOME INOPERATIVE IF THE A/C COMPRESSOR DIODE LEADS ARE SHORTED TO EACH OTHER. IF THE BLUE WIRE TO THE COMPRESSOR FROM THE ELECTRONIC CLIMATE CONTROL (ECC) POWER MODULE IS MISROUTED, IT CAN PULL THE TWO CONNECTING DIODE WIRES TOGETHER, SHORTING OUT THE DIODE. INSULATE AND REROUTE WIRES AS NECESSARY.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.