VENTIPORT APPLIQUE REPLACEMENT. Buick Electra/Park Avenue 1980

For 1990-2009 cars

# VENTIPORT APPLIQUE REPLACEMENT

THE VENTIPORT APPLIQUE ON THE ELECTRA PARK AVENUE FRONT FENDER MOLDING HAS BEEN RELEASED AS A SERVICE PART AND IS AVAILABLE THROUGH GENERAL MOTORS PARTS DIVISION UNDER PART NUMBER 25510207. PRIOR TO ATTACHING A NEW APPLIQUE, WASH THE FRONT FENDER MOLDING AND ADJACENT AREA WITH DETERGENT AND WATER AND WIPE DRY. A.IF APPLIQUE IS DAMAGED: 1.REMOVE DAMAGED APPLIQUE. 2.CLEAN THE SURFACE OF THE MOLDING WITH 3M GENERAL PURPOSE ADHESIVE CLEANER PART NUMBER 8984 OR EQUIVALENT TO REMOVE ADHESIVE OR OTHER FOREIGN MATERIAL. 3.REMOVE THE PROTECTIVE TAPE FROM THE BACK SIDE OF THE NEW APPLIQUE. CENTER APPLIQUE ON FENDER MOLDING SO THAT APPLIQUE RESTS ENTIRELY ON FLAT SURFACE. PRESS FIRMLY IN PLACE APPLYING PRESSURE EVENLY ACROSS ENTIRE APPLIQUE. (SEE ILLUSTRATION). B.IF APPLIQUE IS MISSING: 1.FOLLOW STEPS 2 AND 3 ABOVE.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.