SERVICE GUILD: FRONT KNUCKLE GREASE CAVITY MODIFICATION. Buick Electra/Park Avenue 1988

For 1990-2009 cars

# SERVICE GUILD: FRONT KNUCKLE GREASE CAVITY MODIFICATION

FRONT KNUCKLE CAVITY GREASE FILL OPERATION

#### VEHICLES AFFECTED: 1988 "C" AND "H" CARLINES -----------------

A recent change in the front knuckle cavity eliminated the drain provision. It is important that any time the axle shaft is removed, Cavity A in the illustration be filled 100% full of grease using GM 993037, available thru GMSPO.

#### NOTICE: IF THE HUB BEARING IS REPLACED, THE GREASE WILL COME IN THE SERVICE KIT.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.