SERVICE GUILD: SMU SEC.1B-A/C TORQUE SPECS. Buick Electra/Park Avenue 1990

For 1990-2009 cars

# SERVICE GUILD: SMU SEC.1B-A/C TORQUE SPECS

#### MODELS AFFECTED: 1990 ELECTRA/PARK AVENUE AND LESABRE

The torque specification for the bolt holding the clamp for the refrigerant line routing on Page 1B-28, Figure 25, Item #8, changed from 5.5 N.m (45 lb-in) to 33 N.m (24 lb-ft).

Please update your respective Service Manuals accordingly.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.