DIAGNOSING ENGINE MYSTERY NOISE AT/JUST ABOVE IDLE. Buick Electra/Park Avenue 1985

For 1990-2009 cars

# DIAGNOSING ENGINE MYSTERY NOISE AT/JUST ABOVE IDLE

#### VEHICLES AFFECTED: 1985 'A', and 'C' Models With 3.8L MFI Engines (VIN Code 3) ----------------------------------------------

The following may prove helpful in resolving a particular engine noise condition on the above engines. The noise we refer to, sometimes called 'mystery noise', is tlie result of fore and aft movement of the rod on the crank pin journal.

The noise is normally heard when engirle RPM is just above idle, it's thoroughly warmed up, and under light load (car in gear). The noise can best be described as a light ticking sound much like overhead noise, but appears to come from the bottom part of the engine, and is most pronounced at the rear of the front wheel opening, right side. Removal of the crankshaft balancer and belts will usually greatly reduce the noise level.

A new crankshaft balancer which elimiiiates this noise, through dampening, is available from GM Parts, under part number 25527065.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.