SERVICE GUILD: BROKEN VALVE SPRING CAPS REP. ALL WITH P/N. Buick Electra/Park Avenue 1988

For 1990-2009 cars

# SERVICE GUILD: BROKEN VALVE SPRING CAPS REP. ALL WITH P/N

#### VEHICLES AFFECTED: 1988 'C,E,H'SERIES EQUIPPED WITH 3800 (VIN CODE C) V6 ENGINES

Beginning January 25, 1988, increased strength valve spring caps were released into production for the 3800 engine. All 3800 engines built after the following breakpoints were assembled with the new valve spring caps.

Engine Code Beginning Breakpoint (Engine Build Sequence) ------------ ----------------------- FBA 0305856 FCA 0326238 FDA 0330374

If broken valve spring caps are encountered on an engine assembled prior to the breakpoints, replace all valve spring caps with Part Number 25534605 (12 per engine), available from GMSPO.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.