ENGINE MOUNTING BRACKET REWORK DRILL HOLES. Buick Electra/Park Avenue 1985

For 1990-2009 cars

# ENGINE MOUNTING BRACKET REWORK DRILL HOLES

IF REPLACEMENT OF THE ENGINE MOUNTING BRACKET (P/N 25521356) IS REQUIRED ON THE ABOVE VEHICLES IT MAY BE NECESSARY TO REWORK THE SERVICE PART BY DRILLING TWO ADDITIONAL 7.33/7.22MM HOLES IN THE BRACKET. THESE HOLES ARE NECESSARY FOR MOUNTING THE CATALYTIC CONVERTER AIR INJECTION PIPE AND CHECK VALVE AND WERE NOT INCORPORATED IN SOME EARLY REPLACMENT PARTS STOCK. IF DRILLING THE HOLES IS REQUIRED USE THE OLD BRACKET AS A TEMPLATE.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.