WHEEL ALIGNMENT SPECIFICATIONS REVISIONS TO SERVICE MANUAL. Buick Electra/Park Avenue 1988

For 1990-2009 cars

# WHEEL ALIGNMENT SPECIFICATIONS REVISIONS TO SERVICE MANUAL

WHEEL ALIGNMENT SPECIFICATIONS

#### VEHICLES AFFECTED: 1988 C AND H CARS ----------------- Wheel alignment specifications have changed since the 1988 Chassis Service Manual was published. Use the following specifications when performing a wheel alignment on 1988 C and H cars.

#### FRONT

o Camber +.2 deg. + or - .5 deg.

o Cross Camber 0 deg. + or - .75 deg. (LH Minus RH)

o Caster 3 deg. + or - .5 deg.

o Cross Caster 0 deg. + or - .75 deg. (LH Minus RH)

o Toe (per wheel) 0 deg. + or - .1 deg.

o Sum Toe 0 deg. + or - .2 deg. (LH Plus RH)

o Steering Wheel Angle 0 deg. + or - 3 deg.

#### NOTE: For the Cadillac Deville only.

o Camber Right +0.5 deg. + or - 0.5 deg. Left -0.5 deg. + or - 0.5 deg.

o Cross Camber 0 deg. + or - 0.5 deg. (LH Minus RH)

o Caster 3.0 deg. + or - 1.0 deg.

#### REAR

o Camber -.3 deg. + or - .5 deg.

o Toe (per wheel) .05 deg. + or - .1 deg.

o Sum Toe .1 deg. + or - .2 deg.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.