UPDATE-REMOVAL PROCEDURE EXHAUST MANIFOLD. Buick Electra/Park Avenue 1989

For 1990-2009 cars

# UPDATE-REMOVAL PROCEDURE EXHAUST MANIFOLD

#### VEHICLES AFFECTED: 1989-90 C AND H CARS

This bulletin contains the revised procedure for removing the right side exhaust manifold. This revised procedure replaces the procedure published in Section 6A5A 1989 C-H and Section 6A8 1990 C-H Service Manuals.

Remove or Disconnect

1. Negative battery cable. 2. Spark plug wires from spark plugs. 3. Throttle cable bracket. 4. Crossover pipe heat shield. 5. Transaxle oil level indicator and indicator tube. 6. Oxygen sensor lead. 7. EGR pipe. 8. Two bolts attaching exhaust crossover pipe to manifold. 9. Plastic vacuum tank mounted on cowl. 10. Raise vehicle and suitably support, see Section OA. 11. Catalytic converter heat shield and pipe hanger. 12. Front exhaust pipe to exhaust manifold attaching nuts. 13. Front exhaust pipe from exhaust manifold. 14. Lower vehicle. 15. Engine lift bracket. 16. Exhaust manifold nuts and manifold.

Install or Connect

To complete installation, reverse the removal procedure.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.