WHEEL ALIGNMENT SPECIFICATION REVISED. Buick Electra/Park Avenue 1987

For 1990-2009 cars

# WHEEL ALIGNMENT SPECIFICATION REVISED

#### MODELS AFFECTED: 1987 FRONT WHEEL DRIVE ELECTRAS AND LESABRES

Wheel alignment specifications have changed since the 1987 Chassis Service Manual was published. Use the following specifications when performing a wheel alignment on 1987 front wheel drive Electras and LeSabres:

Front

o Camber +.2 DEG +/- .5 DEG o Cross Camber 0 DEG +/- .75 DEG (left-right) o Caster 2.5 DEG +/- .5 DEG o Cross Caster 0 DEG +/- .75 DEG o Toe (per wheel) 0 DEG +/- .1 DEG o Sum Toe 0 DEG +/- .2 DEG o Steering Wheel Angle 0 DEG +/- 3 DEG

Rear

o Camber -.3 DEG +/- .5 DEG o Cross Camber 0 DEG +/- .75 DEG (left-right) o Toe (per wheel) .05 DEG +/- .1 DEG o Sum Toe .1 DEG +/- .2 DEG

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.