FRONT STRUT DAMPENER SHAFT NUT TORQUE CHANGE. Buick Electra/Park Avenue 1985

For 1990-2009 cars

# FRONT STRUT DAMPENER SHAFT NUT TORQUE CHANGE

#### VEHICLES AFFECTED: 1985 'C' Series Vehicles ------------------------

The front. suspension strut dampener shaft nut torque has been changed from 100 N.m (74 ft. lbs.) to 60 N.m (44 ft.lbs.). This change should be noted on Page 3C(c)-10, Step 7 of the 1985 'C' Series Service Manual.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.