WHEEL ALIGNMENT SPECIFICATIONS REVISIONS TO SERVICE MANUAL. Buick Electra/Park Avenue 1988

For 1990-2009 cars

# WHEEL ALIGNMENT SPECIFICATIONS REVISIONS TO SERVICE MANUAL

#### MODELS AFFECTED: 1988 FRONT WHEEL DRIVE ELECTRAS AND LESABRES

Wheel alignment specifications have changed since the 1988 Chassis Service Manual was published. Use the following specifications when performing a wheel alignment on 1988 front wheel drive Electras and LeSabres:

#### Front

* Camber +.2 DEG. +/- .5 DEG,

* Cross Camber 0 DEG. +/- .75 DEG.

* Caster 3 DEG. +/- .5 DEG.

* Cross Caster 0 DEG. +/- .75 DEG. (LH Minus RH)

* Toe (per wheel) 0 DEG. +/- .1 DEG.

* Sum Toe 0 DEG. +/- .2 DEG. (LH Plus RH)

* Steering Wheel Angle 0 DEG. +/- 3 DEG.

#### Rear

* Camber -.3 DEG. +/- .5 DEG.

* Toe (per wheel) .05 DEG. +/- .1 DEG.

* Sum Toe .1 DEG. +/- .2 DEG.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.