Engine Oil and Oil Filter Replacement. Buick GL7 (Export) 2000

For 1990-2009 cars

### Removal Procedure

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle in General Information.
2. Position the oil drain pan under the engine oil drain plug.
3. Remove the engine oil pan drain plug.
4. Clean and inspect the engine oil pan drain plug, repair or replace if necessary.
5. Clean and inspect the engine oil pan drain plug sealing surface on the oil pan, repair or replace oil pan if necessary.
6. Remove the oil filter.
7. Clean and inspect the oil filter sealing area on the engine block, repair or replace if necessary.

### Installation Procedure

1. Lightly oil the replacement oil filter gasket with clean oil and install the new oil filter.
2. Install the NEW oil filter. Refer to Maintenance Items in Maintenance and Lubrication.

Tighten
Tighten the new oil filter to 3/4 to 1 full turn, after the oil filter gasket contacts the oil filter mounting surface.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

3. Install the engine oil pan drain plug.

Tighten
Tighten the engine oil pan drain plug to 25 N·m (18 lb ft).

4. Remove the oil drain pan.
5. Lower the vehicle.
6. Fill the engine with new engine oil. Refer to Approximate Fluid Capacities , Fluid and Lubricant Recommendations and Explanation of Scheduled Services in Maintenance and Lubrication.
7. Start the engine.
8. Inspect for oil leaks after engine start up.
9. Turn off the engine and allow the oil a few minutes to drain back into the oil pan.
10. Remove the oil level indicator from the oil level indicator tube.
11. Clean off the indicator end of the oil level indicator with a clean paper towel or cloth.
12. Install the oil level indicator into the oil level indicator tube until the oil level indicator handle contacts the top of the oil level indicator tube.
13. Again, remove the oil level indicator from the oil level indicator tube keeping the tip of the oil level indicator down.
14. Check the level of the engine oil on the oil level indicator.
15. If necessary, adjust the oil level by adding or draining the engine oil.