Crankshaft Front Oil Seal Installation. Buick GL7 (Export) 2001

For 1990-2009 cars

1. Lubricate the new crankshaft front oil seal with Chassis Grease GM P/N 1051344 or equivalent.

Important: Tap the oil seal in until its surface is flush with the crankshaft front oil seal retainer edge.

2. Using a hammer and an appropriate driver, lightly tap the crankshaft front oil seal into place.
3. Install the crankshaft balancer. Refer to Crankshaft Pulley Installation .