Steering Column Trim Covers - Assemble - Off Vehicle. Buick GL7 (Export) 2000

For 1990-2009 cars

### Assembly Procedure

#### Tools Required

J 41352 Modular Column Holding Fixture

1. Install the shroud protector (1) to the lower shroud (2).
2. Install the upper shroud (2) onto the steering column.
3. Slide the shift lever seal down the shift lever and install into the upper shrouds (2).

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

4. Secure the upper shroud (2) using 1 TORX® head screw (1).

Tighten
Tighten the screw to 1.5 N·m (13 lb in).

5. Install the lower shroud (2) and secure by using 2 pan head tapping screws (1).

Adjust the shift lever seal into the shroud.

Tighten
Tighten the screws to 3.5 N·m (31 lb in).

6. Install the tilt lever into the shroud.
7. Take the column out from the J 41352 .
8. Remove the top piece of J 41352 from the steering column.
9. Remove J 41352 from the vise.