Steering Column Tilt Head Housing - Assemble - Off Vehicle. Buick GL7 (Export) 2000

For 1990-2009 cars

### Assembly Procedure

#### Tools Required

J 23653-SIR Lock Plate Compressor

1. Align the race and upper shaft assembly (1) to the 12 o'clock position.
2. Put the lock cylinder in the lock position and remove the key.
3. Install the inner race (5).
4. Install the upper bearing inner race seat (4).
5. Install the upper bearing spring (3).
6. Lubricate the turn signal cancel cam assembly (2).
7. Install the turn signal cancel cam assembly (2).
8. Install the shaft lock shield assembly (1).
9. Install the bearing retaining using J 23653-SIR .
10. Remove J 23653-SIR from the steering column.
11. Install the SRS coil assembly. Refer to Inflatable Restraint Steering Wheel Module Coil Assemble - Off Vehicle .