Drive Belt Tensioner Replacement. Buick GL7 (Export) 2000

For 1990-2009 cars

### Removal Procedure

1. Remove the drive belt. Refer to Drive Belt Replacement .
2. Remove the drive belt tensioner bolt.
3. Remove the drive belt tensioner.

### Installation Procedure

1. Install the drive belt tensioner.
2. Install the drive belt tensioner bolt.

Tighten
Tighten the drive belt tensioner bolt to 50 N·m (37 lb ft).

3. Install the drive belt. Refer to Drive Belt Replacement .