Evaporative Emission Canister Purge Solenoid Valve Replacement. Buick GL7 (Export) 2000

For 1990-2009 cars

### Removal Procedure

1. Turn OFF the ignition.
2. Note the position of the EVAP hoses for installation.
3. Disconnect the electrical connector and hoses from the EVAP canister purge valve.
4. Remove the bolt from the valve mounting bracket.
5. Remove the EVAP purge valve.

### Installation Procedure

1. Position the EVAP canister purge valve on the manifold.
2. Install the bolt and secure the EVAP canister purge valve.
3. Connect the electrical connector and the hoses to the valve.