Steering Column Trim Covers - Disassemble - Off Vehicle. Buick GL7 (Export) 2000

For 1990-2009 cars

### Disassembly Procedure

#### Tools Required

J 41352 Modular Column Holding Fixture

1. Place the bottom of J 41352 into a vise.
2. Set the steering column in the J 41352 .
3. Place the top piece of J 41352 onto the column.
4. Pull the tilt lever out from the lower shroud.
5. Remove 2 pan head tapping screws (2) from the lower shroud (1).
6. Remove the lower shroud (1).
7. Remove 1 TORX® head screw (1) from the upper shroud (2).
8. Slide the shift lever seal up the shift lever.
9. Remove the upper shroud (2).
10. Remove the shroud protector (1) from the lower shroud (2).