Sliding Door Inside Handle Replacement. Buick GL7 (Export) 2000

For 1990-2009 cars

### Removal Procedure

#### Tools Required

J 38864 Counterbalance Spring Removal and Installation Tool

Use J 38864 to remove the sliding door inside handle from the door.

### Installation Procedure

1. Load the door inside handle clip into the handle with the open end facing down.
2. Align the door inside handle with the shaft on the sliding door.
3. Press firmly in order to seat the sliding door inside handle.