Door Trim Panel Replacement. Buick GL7 (Export) 2000

For 1990-2009 cars

### Removal Procedure

1. Position the window all the way down.
2. Remove the outer belt sealing strip screws.
3. Use your fingertips in order to pull the sealing strip from the door flange.

### Installation Procedure

1. Position the sealing strip to the door flange by pressing the strip in place.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

2. Install the outer belt sealing strip screws.

Tighten
Tighten the outer belt sealing strip screws to 1.5 N·m (13 lb in).