High Beam Indicator Always On. Buick GL7 (Export) 2000

For 1990-2009 cars

Step | Action | Yes | No
--- | --- | --- | ---
1 | Did you perform the Lighting System Diagnostic System Check? | Go to Step 2 | Go to Diagnostic System Check - Lighting Systems
2 | Are both turn signal indicators on also? | Go to Step 3 | Go to Step 4
3 | Repair the open in the ground circuit of the IPC. Refer to Wiring Repairs in Wiring Systems. Is the repair complete? | Go to Step 6 | --
4 | Are the high beam headlamps illuminated? | Go to Headlamp Low or High Beams Always On | Go to Step 5
5 | Replace the IPC. Refer to Instrument Cluster Replacement in Instrument Panel, Gauges, and Console. Important: Perform the set up procedure for the IP. Did you complete the replacement and the set up procedure? | Go to Step 6 | --
6 | Operate the system in order to verify the repair. Did you correct the condition? | System OK | Go to Step 2