Instrument Panel Inflatable Restraint Module Replacement. Buick GL7 (Export) 2000

For 1990-2009 cars

### Removal Procedure

Caution: When you are carrying an undeployed inflator module:

• | Do not carry the inflator module by the wires or connector on the inflator module

• | Make sure the bag opening points away from you

When you are storing an undeployed inflator module, make sure the bag opening points away from the surface on which the inflator module rests. When you are storing a steering column, do not rest the column with the bag opening facing down and the column vertical. Provide free space for the air bag to expand in case of an accidental deployment. Otherwise, personal injury may result.
1. Disable the SIR system. Refer to Disabling the SIR System .
2. Remove the instrument panel (IP) compartment and the lamp electrical connector. Refer to Instrument Panel Compartment Replacement in Instrument Panel, Gauges and Console.
3. Remove the pigtail harness clips from the IP carrier bracket.
4. Remove the IP module mounting fasteners (4).
5. Remove the IP module bolts (5) that attach the IP module to the cross-car beam.
6. Remove the inflatable restraint IP module (1).
7. Fully deploy the module before disposal. If the module was replaced under warranty, fully deploy and dispose of the module after the required retention period. Refer to Inflator Module Handling, Shipping, and Scrapping .

### Installation Procedure

1. Install the inflatable restraint IP module (1).
2. Install the inflatable restraint IP module bolts (5).

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

3. Install the inflatable restraint IP module mounting fasteners (4).

Tighten
Tighten fasteners to 10 N·m (89 lb in).

4. Install the pigtail harness clips to the IP carrier bracket.
5. Install the electrical connector to the IP compartment lamp and install the IP compartment. Refer to Instrument Panel Compartment Replacement in Instrument Panel, Gauges and Console.
6. Enable the SIR system. Refer to Enabling the SIR System .