Hood Rear Seal Replacement. Buick GL7 (Export) 2000

For 1990-2009 cars

### Removal Procedure

1. Open and suitably support the hood.
2. Remove the hood rear weather-strip from the flange.
3. Remove the hood rear outer seals from the fenders.
4. Clean the surface of the fender in the area of the hood outer seals in order to ensure proper adhesion of adhesive.

### Installation Procedure

1. Apply glue if you are reusing the old hood rear weather-strip.
2. Install the hood rear weather-strip to the flange.
3. Install the hood rear outer seals to the fenders.
4. Press in order to secure the seal adhesive to the fender.
5. Close the hood.