Crankcase Ventilation System Description. Buick GL7 (Export) 2000

For 1990-2009 cars

### General Description

A crankcase ventilation system is used to consume crankcase vapors in the combustion process instead of venting the vapors to atmosphere. Fresh air from the throttle body is supplied to the crankcase, mixed with blow-by gases and then passed through a positive crankcase ventilation (PCV) valve into the intake manifold.

### Operation

The primary control is through the positive crankcase ventilation (PCV) valve which meters the flow at a rate depending on the inlet vacuum. To maintain idle quality, the PCV valve restricts the flow when the inlet vacuum is high. If abnormal operating conditions arise, the system is designed to allow excessive amounts of blow-by gases, to backflow through the crankcase vent into the throttle body to be consumed by normal combustion.

### Results of Incorrect Operation

A plugged valve may cause the following conditions:

• | A rough idle condition

• | A stalling or slow idle speed condition

• | Any oil leaks

• | Any sludge in the engine

A leaking valve would cause the following conditions:

• | A rough idle

• | Stalling

• | A high idle speed

### Functional Check of PCV valve

If an engine is idling rough, check for a plugged PCV valve. Replace the valve if necessary. Use the following procedure:

1. Remove the PCV valve from the intake manifold.
2. Shake the valve and listen for the rattle of the needle inside the valve.
3. If the valve does not rattle, replace the valve.

With this system, any blow-by in excess of the system capacity is exhausted into the intake manifold and is drawn into the engine.

Proper operation of the crankcase ventilation system is dependent upon a sealed engine. If oil sludging or dilution is noted, and the crankcase ventilation system is functioning properly, check the engine for a possible cause, and correct the condition to ensure that the system will function as intended.