Rear Side Door Center Roller Bracket Replacement. Buick GL7 (Export) 2000

For 1990-2009 cars

### Removal Procedure

1. Open the sliding door in order to gain access to the center roller bracket pin.
2. Support the rear of the sliding door.
3. Remove the pin from the center roller bracket.
4. Position the center roller bracket to the front radius of the sliding door center track.
5. Remove the right rear quarter trim. Refer to Rear Quarter Lower Trim Panel Replacement .
6. Lift the center roller bracket upwards and remove the bracket from the center track.

### Installation Procedure

1. Position the sliding door center roller bracket to the front radius of the sliding door center track.
2. Lower the sliding door center roller bracket to sliding door center track down and into the sliding door center track.
3. Place the sliding door center track roller bracket in the front of the sliding door center track.
4. Pull the sliding door center roller bracket towards the front of the sliding door center track.
5. Position the sliding door center roller bracket at the front of the track, 25 mm (1 in) from the front radius of the center track.
6. Position the sliding door center roller bracket to the rear of the track or until the pin holes are aligned.
7. Install the pin to the sliding door center roller bracket.
8. Remove the support from the power sliding door.
9. Manually open and close the rear sliding door in order to verify the door's fit and the door's latch/unlatch operation.
10. Install the right rear quarter trim. Refer to Rear Quarter Lower Trim Panel Replacement .
11. Lubricate the front radius of the center track.