Exhaust Manifold Removal. Buick GL7 (Export) 2000

For 1990-2009 cars

## Exhaust Manifold Removal Left Side VIN M

1. Remove the exhaust manifold heat shield bolts.
2. Remove the exhaust manifold heat shield.
3. Remove the left side spark plugs.
4. Remove the exhaust manifold nuts.
5. Remove the exhaust manifold.
6. Remove the exhaust manifold gasket.

## Exhaust Manifold Removal Right Side

1. Remove the exhaust manifold heat shield bolts.
2. Remove the exhaust manifold heat shields.
3. Remove the exhaust manifold nuts.
4. Remove the exhaust manifold.
5. Remove the exhaust manifold gasket.