Generator Bracket Replacement. Buick GL7 (Export) 2000

For 1990-2009 cars

### Removal Procedure

1. Remove the generator. Refer to Generator Replacement .
2. Remove the drive belt tensioner. Refer to Drive Belt Tensioner Replacement in Engine Mechanical.
3. Remove the generator bracket bolts.
4. Remove the generator bracket.

### Installation Procedure

1. Install the generator bracket.
2. Install the generator bracket bolts.

Tighten
Tighten the generator bracket bolts in the sequence shown to 50 N·m (37 lb ft).

3. Install the drive belt tensioner. Refer to Drive Belt Tensioner Replacement in Engine Mechanical.
4. Install the generator. Refer to Generator Replacement .