Driver or Passenger Seat Cushion Frame Replacement. Buick GL7 (Export) 2000

For 1990-2009 cars

### Removal Procedure

1. Remove the seat cushion cover. Refer to Front Seat Cushion Cover Replacement .
2. Remove the seat cushion frame from the seat cushion pad.
3. Unhook the seat cushion support from the frame.

### Installation Procedure

1. Hook the seat cushion support to the frame.
2. Install the seat cushion frame to the seat cushion pad.
3. Install the seat cushion cover. Refer to Front Seat Cushion Cover Replacement .