Engine Flywheel Replacement. Buick GL7 (Export) 2000

For 1990-2009 cars

### Removal Procedure

1. Remove the automatic transaxle. Refer to Transmission Replacement in Automatic Transaxle.
2. Remove the engine flywheel. Refer to Engine Flywheel Removal .
3. Clean the engine flywheel bolt threads and bolt holes.
4. Clean and inspect the engine flywheel. Refer to Engine Flywheel Cleaning and Inspection .

### Installation Procedure

1. Install the engine flywheel. Refer to Engine Flywheel Installation .
2. Install the automatic transaxle. Refer to Transmission Replacement in Automatic Transaxle.