Fuel Pump Strainer Replacement. Buick GL7 (Export) 2000

For 1990-2009 cars

### Removal Procedure

Important: Always maintain cleanliness when servicing fuel system components.

1. Remove the fuel sender assembly. Refer to Fuel Sender Assembly Replacement .
2. Note the strainer (3) position for future reference.
3. Support the reservoir with one hand and grasp the strainer with the other hand.
4. Use a screwdriver to pry the strainer ferrule off the reservoir.
5. Discard the strainer.

### Installation Procedure

1. Install the new strainer (4) to the reservoir.
2. Support the reservoir with one hand and grasp the strainer with the other hand twisting the strainer into position.
3. Install the fuel sender assembly. Refer to Fuel Sender Assembly Replacement .