Inflatable Restraint Steering Wheel Module Coil Disassemble - Off Vehicle. Buick GL7 (Export) 2000

For 1990-2009 cars

### Disassembly Procedure

1. Remove the upper and lower shrouds. Refer to Steering Column Trim Covers - Disassemble - Off Vehicle .
2. Pop the wire harness assembly (4) out of the wire harness strap (5).
3. Remove the wire harness straps (3) from the wire harness assembly (4).
4. Remove 1 wire harness strap (2) from the upper tilt head assembly (1).
5. Remove the snap ring (1).
6. Remove the SRS coil assembly (2).
7. Remove the wave washer (3).