Wheelhouse Splash Shield Replacement. Buick GL7 (Export) 2000

For 1990-2009 cars

### Removal Procedure

#### Tools Required

J 38778

1. Remove the bolts/screws from the fender splash shield.
2. Use J 38778
3. Remove the fender splash shield from the fender.

### Installation Procedure

1. Align the locating pins on the fender splash shield into the holes in the fender.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

2. Install the bolts/screws to the fender splash shield.

Tighten
Tighten the bolts/screws to 2 N·m (18 lb in).

3. Install the push-in retainer to the lower fender splash shield at the rocker panel.