Automatic Transmission Range Selector Lever Replacement. Buick GL7 (Export) 2000

For 1990-2009 cars

### Removal Procedure

1. Remove the throttle body air inlet duct. Refer to Air Cleaner Assembly Replacement in Engine Controls.
2. Remove the automatic transaxle range selector lever cable from the cable lever.
3. Remove the automatic transaxle range selector lever nut.
4. Remove the automatic transaxle range selector lever.

### Installation Procedure

1. Install the automatic transaxle range selector lever.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

2. Install the automatic transaxle range selector lever nut.

Tighten
Tighten the automatic transaxle range selector lever nut to 32 N·m (23 lb ft).

3. Install the automatic transaxle range selector lever cable to the automatic transaxle range selector lever.
4. Install the throttle body air inlet duct. Refer to Air Cleaner Assembly Replacement in Engine Controls.