Front Side Door Lock Actuator Replacement. Buick GL7 (Export) 2000

For 1990-2009 cars

### Removal Procedure

1. Remove the door module. Refer to Front Door Module Replacement .
2. Remove the front door lock. Refer to Front Side Door Lock Replacement .
3. Remove the lock actuator from the front door lock.

### Installation Procedure

1. Install the lock actuator to the front door lock.
2. Install the front door lock. Refer to Front Side Door Lock Replacement .
3. Install the door module. Refer to Front Door Module Replacement .