ASHTRAY COVER DISTORTING INSTALL NEW COVER. Buick Reatta 1988

For 1990-2009 cars

# ASHTRAY COVER DISTORTING INSTALL NEW COVER

#### VEHICLES AFFECTED: 1988-89 E

Some 1988-1989 Oldsmobile Trofeos and 1989 Toronados and Trofeos may experience distortion and warping of the passenger side ash tray cover in the door armrest. This condition may be caused by natural interior heat load and results from the use of a material with low heat resistance for the ash tray covers. The affected covers are black, moulded plastic with an applique. Chrome plated covers are not affected.

To repair this condition replace only the ashtray cover using the following part and procedure:

Ashtray Lid: P/N 20726767

Tools Required: Torx-head (Tl5) screwdriver Small pair side cutters Needle-nose pliers

1. Using a Torx-head screwdriver (Tl5), remove the switch plate retention screw located at the front of the plate under the ashtray cover.

2. Lift up on the front of the switch plate and pull forward slightly to disengage from the armrest.

3. Disconnect switches.

4. Turn switch plate over. Remove spring from ashtray cover. Remove ash receptacle if necessary.

5. Using a small pair of side cutters, cut off the cover stop (the finger which holds the spring) to allow cover removal.

Disengage the cover from the switch plate by flexing the cover in the centre, rear. Refer to Figure 1, a and b. DO NOT DISCARD COVER UNTIL AFTER NEXT STEP.

6. Position new cover on switch plate. Remove spring pin from old cover with pliers. Press through hole in switch plate into the new cover. Refer to Figure 2, a and b.

7. Reassemble the spring to switch plate and cover.

8. Reassemble the switch plate to the armrest. Replace ash receptacle.

Use most applicable Labour operations and Time from the Canadian Labour Time Guide.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.