HIGH EFFORT TO OPEN REAR COMPARTMENT LID. Buick Reatta 1988

For 1990-2009 cars

# HIGH EFFORT TO OPEN REAR COMPARTMENT LID

#### MODELS AFFECTED: 1988 REATTA

Some early built 1988 Reattas may require a high effort to lift the rear compartment lid. This condition can be corrected by installing new design supports (2 required), Part Number 20731751. Parts are currently available from GMSPO.

The following information will help in identifying the first and second designs:

Design Part Number Type ------ ----------- ---- First 20588231 Gas Filled Second 20721751 Oil Filled

The second design support must be mounted in an inverted position from the original first design support. See Figures 1 and 2 for correct mounting pcsitions.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.