DOOR LOCK MODULE RATTLE (INSTALL NEW RIVET). Buick Reatta 1990

For 1990-2009 cars

# DOOR LOCK MODULE RATTLE (INSTALL NEW RIVET)

#### MODELS AFFECTED: 1990 RIVIERA

This bulletin is being revised to increase the labor time from .3 hour to .5 hour. Please discard bulletin 90-10-10.

Some 1990 E/K may experience a condition of a rattle from the front door during closing. This condition may be caused by loose rivets securing the lock module to the door inner panel.

To repair this condition use the following procedure:

1. Remove the door trim panel and noise suppressing foam pad.

2. Drill and insert an additional 3/16" x 1/8" rivet to the locations specified on the attached artwork. Refer to Figures 1 and 2.

3. Install the door trim panel and noise suppressing foam pad.

For warranty purposes use Labor Operation T6405 at .5 hour for the left side, and T6406 at .5 hour for the right side.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.