RIVIERA BODYSIDE MOLDING THICKNESS INCREASED-NEW PARTS. Buick Reatta 1989

For 1990-2009 cars

# RIVIERA BODYSIDE MOLDING THICKNESS INCREASED-NEW PARTS

#### MODELS AFFECTED: 1989 RIVIERAS

The body side moldings used on Rivieras were originally manufactured in stainless steel in a thickness of .46-.50mm. To improve the ability to resist denting, a new molding is being released for service. The new molding has a gage thickness of .54-.60mm. Part numbers for these moldings are listed below:

Front Fender Right/Left 20729258/-9 Door Right/Left 12500994/-3 Rear Quarter Right/Left 12394244/-5

Parts are currently available from GMSPO.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.