REAR COMPARTMENT ACCESS DOOR RATTLE/NEW LATCH PIN. Buick Reatta 1988

For 1990-2009 cars

# REAR COMPARTMENT ACCESS DOOR RATTLE/NEW LATCH PIN

#### MODELS AFFECTED: 1988-89 REATTA

If an owner should comment about a rattle in the area of the rear compartment access door, it can sometimes be corrected by installing a new coated rear compartment access door latch pin, part number 20702007. (2 required)

Use the following procedure to install the latch pins:

1. Open the rear access door and locate the two (2) latch pins at the upper corners of the opening.

2. Holding the latch pin in position with a 14mm wrench, reach through the opening to remove the 13mm nut and washer.

3. Remove the latch pins and replace with part number 20702007. Reinstall the washers and nuts.

Parts are currently available from GMSPO.

#### WARRANTY INFORMATION:

Labor Operation No.: T6478 Labor Operation Time: .2 hr.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.