SERVICE GUILD: SMU STEERING WHEEL REMOVAL. Buick Reatta 1989

For 1990-2009 cars

# SERVICE GUILD: SMU STEERING WHEEL REMOVAL

#### SUBJECT: STEERING WHEEL REMOVAL, WITH ACCESSORY CONTROLS

#### VEHICLES AFFECTED: 1989 W CARS WITH UK3 OPTION

#### SERVICE MANUAL UPDATE

The following bulletin is for the 1989 Pontiac Grand Prix and Buick Regal, this information has been printed in the Oldsmobile Cutlass Supreme Service Manual.

The following Notice should be inserted following Steering Wheel Removal, of Section 3F1 and 3F2.

#### NOTICE: WHEN REMOVING A STEERING WHEEL WITH REDUNDANT ELECTRONIC ACCESSORY CONTROLS IN THE HUB, CARE MUST BE TAKEN TO AVOID DAMAGE TO ELECTRONIC CIRCUITS. WHEEL PULLER BOLTS, USED WITH SPECIAL TOOL J 1859-03, SHOULD BE TURNED INTO STEERING WHEEL HUB NO MORE THAN FIVE COMPLETE TURNS. THIS WILL PREVENT BOLT CONTACT WITH SENSITIVE ELECTRONIC CIRCUITS.

The notice will appear on the following pages:

1989 Grand Prix Page 3F2-1 1989 Regal Page 3F1-1

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.