GAP AT GLOVE BOX DOOR TO I/P (ADJUST GLOVE BOX DOOR). Buick Roadmaster 1994

For 1990-2009 cars

# GAP AT GLOVE BOX DOOR TO I/P (ADJUST GLOVE BOX DOOR)

#### SUBJECT: GAP AT GLOVE BOX DOOR TO INSTRUMENT PANEL (ADJUST GLOVE BOX DOOR)

#### MODELS: 1994 BUICK ROADMASTER

#### CONDITION:

OBJECTIONABLE GAP AT TOP LEFT SIDE OF GLOVE BOX DOOR TO INSTRUMENT PANEL.

#### CORRECTION:

LOOSEN SCREW/BOLT #2 TO INSTRUMENT PANEL LOWER BRACE #1 WHERE IT ATTACHES TO THE CARRIER BETWEEN THE GLOVE BOX DOOR AND THE ASHTRAY, SEE FIGURE 1.

PUSH LOWER EDGE OF GLOVE BOX DOOR FORWARD (TOWARDS FRONT OF VEHICLE) AND TIGHTEN SCREW/BOLT.

#### WARRANTY INFORMATION:

FOR VEHICLES REPAIRED UNDER WARRANTY, USE: LABOR OPERATION: T3413 LABOR OPERATION: 0.2 HR.

FIGURES: 0

GENERAL MOTORS BULLETINS ARE INTENDED FOR USE BY PROFESSIONAL TECHNICIANS, NOT A "DO-IT-YOURSELFER". THEY ARE WRITTEN TO INFORM THOSE TECHNICIANS OF CONDITIONS THAT MAY OCCUR ON SOME VEHICLES, OR TO PROVIDE INFORMATION THAT COULD ASSIST IN THE PROPER SERVICE OF A VEHICLE. PROPERLY TRAINED TECHNICIANS HAVE THE EQUIPMENT, TOOLS, SAFETY INSTRUCTIONS AND KNOW-HOW TO DO A JOB PROPERLY AND SAFELY. IF A CONDITION IS DESCRIBED, DO NOT ASSUME THAT THE BULLETIN APPLIES TO YOUR VEHICLE, OR THAT YOUR VEHICLE WILL HAVE THAT CONDITION. SEE A GENERAL MOTORS DEALER SERVICING YOUR BRAND OF GENERAL MOTORS VEHICLE FOR INFORMATION ON WHETHER YOUR VEHICLE MAY BENEFIT FROM THE INFORMATION.

COPYRIGHT 1993 GENERAL MOTORS CORPORATION. ALL RIGHTS RESERVED.