Clean Air Cover and Gasket Replacement. Buick Roadmaster 1996

For 1990-2009 cars

### Removal Procedure

1. Remove the resonator.
2. Remove the clean air cover attaching screws.
3. Remove the clean air cover and the gasket.
4. Discard the gasket.
5. Clean the gasket sealing surfaces.

### Installation Procedure

1. Install a new gasket.
2. Install the clean air cover.
3. Install the clean air cover attaching screws.

Tighten
Tighten the clean air cover attaching screws to 3.2 N·m (28 lb in).

4. Install the resonator.