Engine Flywheel Replacement. Buick Roadmaster 1996

For 1990-2009 cars

### Removal Procedure

1. Remove the transmission. Refer to Transmission Replacement in Automatic Transmission.
2. Remove the flywheel bolts.
3. Remove the flywheel.
4. Clean the mating surfaces of the crankshaft and the flywheel.
5. Remove any burrs.
6. Inspect the flywheel for worn or broken teeth and cracks.

### Installation Procedure

1. Install the flywheel.
2. Install the flywheel bolts.

Tighten
Tighten the flywheel bolts to 100 N·m (74 lb ft).

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

3. Install the transmission. Refer to Transmission Replacement in Automatic Transmission.